A2G-mini: Control of  
filter pressure in limited space

Klingenberg, June 2017.

The new A2G-mini differential pressure gauge from WIKA has been specifically designed for small and medium-sized central ventilation and air-conditioning units. With a nominal size of   
63 mm and an insertion depth of 32 mm, it can be fitted in the tightest of surroundings.

The A2G-mini has been developed with a view to the EU directive for energy-efficient ventilation and air-conditioning systems: From January 1st, 2018, all central units with an air flow of more than 1,000 m³/h must have filter pressure monitoring.

The new differential pressure gauge indicates rising pressure loss reliably and in an easily readable format. It is available with four measuring ranges from 0 … 250 Pa to 0 … 1,000 Pa. The pressure gauge is completely silicone-free and thus fulfils the requirements of ISO 846 (microbial metabolic potential). With IP68 ingress protection and a UV-stabilized window it is also suitable for use in outdoor areas.

Number of characters: 934

Key word: A2G-mini

**WIKA company photograph:**

Differential pressure gauge A2G-mini



**Edited by:**

WIKA Instruments Ltd.

3103 Parsons Road

Edmonton, AB T6N 1C8

Canada

Tel. (+1) 780 463-7035

Fax (+1) 780 462-0017

E-mail [marketing.ca@wika.com](mailto:marketing.ca@wika.com)

[www.wika.ca](http://www.wika.ca)

WIKA press release 11/2017