Universal process transmitter

with global hazardous area approvals

Klingenberg, June 2015.

The safety of the UPT-2x process transmitter from WIKA is certified globally: The universal instrument has achieved approvals for use in hazardous areas in accordance with IECEx, ATEX and now also EAC.

The multi-functional UPT-2x is a solution for tasks in pressure, level and volume measurement. Its sensor, with a measuring range between 0 ... 400 mbar and 0 ... 1000 bar depending on the requirement, operates with an accuracy of up to 0.1 % of the measuring span. For applications in the pharmaceutical and food industries, flush-mounting versions are available. The electronics are protected by a conductive plastic case, or optionally by a stainless steel case in hygienic design.

The measuring ranges of the UPT-2x are freely scalable and can therefore be adjusted to individual measurement tasks. An intuitive-to-use menu in accordance with the HART®-v7 standard and the integrated display make programming easier. With its handling without the need for tools, its high long-term stability and its universal application possibilities, the UPT-2x is also a cost-effective solution.

Number of characters: 1086

Key word: UPT-2x

**WIKA company photograph:**

WIKA process transmitter UPT-2x

****

**Edited by:**

WIKA Instruments Ltd.

3103 Parsons Road

Edmonton, AB T6N 1C8 Canada

Tel. (+1) 780 463-7035

Fax (+1) 780 462-0017

E-mail marketing.ca@wika.com

[www.wika.ca](http://www.wika.ca)

WIKA press release 14/2015